{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["CO Reference Architecture","OSP New Products"],"not_rendered":{"images":9},"read":"whole","date_system":"1900"}

{"sheet":"CO Reference Architecture","index":0,"n_rows":92,"n_cols":9,"rows_kept":92,"merged":[[0,1,0,2],[4,0,6,7],[9,0,9,8],[19,0,19,8],[28,0,28,8],[36,0,36,8],[51,0,51,8],[62,0,62,8],[73,0,73,8],[81,0,81,8],[89,0,90,7],[91,0,92,7]]}
["Name:"]
["Quote Number:","2024-116446"]
["Opportunity Name:","Central Office Reference Architecture"]
["Comments:"]
["The below bill of materials is provided for reference based upon an example central office build-out to support a community with approximately 10,000 locations passed. Quantities and styles will vary based upon the size and architecture for the build-out, as well as numerous other factors."]
[]
[]
[]
["Reference","Line","Part Number","Description","Comments","Qty","UOM","Notes","More Information"]
["Entrance Splice"]
["HD Fusion",1,"FWMHSSGS-6912","Fiber Wallmount Hyper Scale Splicing Enclosure Gray, With Split Doors - 6912 Fiberser Wallmount Hyper Scale Splicing Enclosure Gray, With Split Doors - 3456 Fibers","",1,"Piece","","Panduit.com product page"]
["HD Fusion",2,"FWMHSSGS-3456","Fiber Wallmount Hyper Scale Splicing Enclosure Gray, With Split Doors - 3456 Fibers","",1,"Piece","","Panduit.com product page"]
["HD Fusion",3,"FST48","HD Fusion Splice Tray Kit","",24,"Piece","","Panduit.com product page"]
["HD Fusion",4,"FWMHSS-ICAK","INCOMING CABLE ANCHOR KIT  ","",4,"Piece","","Panduit.com product page"]
["HD Fusion",5,"FWMHSS-CG2135","CABLE GLAND 21MM – 35MM ","",8,"Piece","","Panduit.com product page"]
["HD Fusion",6,"FWMHSSG-ICB","FIBER WALL MOUNT ENCLOSURE INCOMING CABLE BRACKET KIT - Gray","",4,"Piece","","Panduit.com product page"]
["HD Fusion",7,"ACGK","Armor Cable Grounding Kits","",4,"Kit","","Panduit.com product page"]
["HD Fusion",8,"FWMHSSG-GROUND","FIBER WALL MOUNT ENCLOSURE GROUNDING BRACKET - Gray","",1,"Piece","","Panduit.com product page"]
[]
["Equipment Racks"]
["Racks & CM",9,"R2P","Standard Rack - 84\" High (2134mm)","",7,"Piece","","Panduit.com product page"]
["Racks & CM",10,"PR2VD06","PATCHRUNNER2 VERTICAL MANAGER AND DOORS, 6in WIDE, 7ft TALL, FRONT AND REAR","",2,"Piece","","Panduit.com product page"]
["Racks & CM",11,"PR2VD08","PATCHRUNNER2 VERTICAL MANAGER AND DOORS, 8in WIDE, 7ft TALL, FRONT AND REAR","",7,"Piece","","Panduit.com product page"]
["Racks & CM",12,"AR4P","45RU 4-Post Rack, adjustable depth 23\"- 42\", threaded rails, black","",3,"Piece","","Panduit.com product page"]
["Racks & CM",13,"PR2VFD08","PATCHRUNNER2 VERTICAL MANAGER AND DOOR, 8in WIDE, 7ft TALL, FRONT ONLY","",4,"Piece","","Panduit.com product page"]
["Racks & CM",14,"XG74522BS0030","FlexFusion™ Cabinet, 700mm x 45RU x 1200mm, Black, Hardware Mount Rail, Top Cap w/ Brush Seal, Single Hinge Perforated Front Door, Split Perforated Rear Door, Standard Locks, Left and Right Side Panels, One Set Short Cable Mgmt Fingers, Left and Right PDU Brackets, Casters","",3,"Piece",1,"C-RKCAB-XG-MODEL-XB--ENG.pdf"]
["Racks & CM",15,"PR2HF1","PatchRunner2 Horizontal Cable Manager, 1RU tall, Magnetic Cover",null,10,"Piece",null,"Panduit.com product page"]
[]
["Cable Routing"]
["Wire Basket",16,"PWB4X12BL","Wire Basket 4\" H x 12\" W , Black Powdered Coated","",6,"Piece","","Panduit.com product page"]
["Wire Basket",17,"PWBTB12BL","Trapeze Bracket 12\", BL , Panduit Wire Basket","",13,"Piece","","Panduit.com product page"]
["Wire Basket",18,"PWBSPLBL","Panduit Wire Basket Bolted Style Splice, Black, 50 Pieces","",20,"Piece","","Panduit.com product page"]
["Wire Basket",19,"PWBWMWBL","Panduit Wire Basket Wall Termination Bracket, Wide, Black, 2 Pieces","",4,"Piece","","Panduit.com product page"]
["Wire Basket",20,"PWBCB12BL","Cantilever Bracket 12\", BL, Panduit Wire Basket","",5,"Piece","","Panduit.com product page"]
["Wire Basket",21,"PWBPF4X12BL","Formed Tee Fitting 4\" H x 12\" W, Black","",4,"Piece","","Panduit.com product page"]
[]
["Fiber Routing"]
["Fiber Routing",22,"FRBC6X4LYL","Coupler, 6\" x 4\" (150mm x 100mm), FiberRunner, YL","",14,"Piece","","Panduit.com product page"]
["Fiber Routing",23,"FR6X4YL10","Channel, 6\" x 4\" (150mm x 100mm), 10', FiberRunner, YL","",7,"Piece","","Panduit.com product page"]
["Fiber Routing",24,"FRBC4X4LYL","Coupler, 4\" x 4\" (100mm x 100mm), FiberRunner, YL","",14,"Piece","","Panduit.com product page"]
["Fiber Routing",25,"CLT150F-X4","Corr. Loom Tubing Slit, 1.50\" (38.1mm) X 10' (3.0m), Yellow","",3,"Roll","","Panduit.com product page"]
["Fiber Routing",26,"FRHC6YL10","Channel Cover, Hinged, Snap-On, 6\" x 4\" (150mm x 100mm), 10', FiberRunner, YL","",5,"Piece","","Panduit.com product page"]
["Fiber Routing",27,"FR6TRBE12","Bracket, Existing 1/2\" Thr. Rod QuikLock for 4\" x 4\" & 6\" x 4\" FiberRunner","",13,"Piece","","Panduit.com product page"]
["Fiber Routing",28,"FRSPJ4X4LYL","Spill-Over Junction Fitting with 4x4 Exit","",14,"Piece","","Panduit.com product page"]
["Fiber Routing",29,"FRIDT4X4LYL","Fitting, 2-Port Spillout to 1.5\" (38mm) Inside Diameter Corrugated Tubing, YL","",14,"Piece","","Panduit.com product page"]
["Fiber Routing",30,"FRSPJC46LYL","Spill-Over Junction with 4x4 Exit Cover, 6x4 Channel","",14,"Piece","","Panduit.com product page"]
["Fiber Routing",31,"FR6LB","Bracket, \" L\" Wall Mount for 4\" x 4\" & 6\" x 4\" FiberRunner","",7,"Piece","","Panduit.com product page"]
["Fiber Routing",32,"FRT6X4LYL","Fitting, Horizontal Tee, 6\" x 4\" (150mm x 100mm), FiberRunner, YL","",4,"Piece","","Panduit.com product page"]
["Fiber Routing",33,"FRTSC6LYL","Split Cover, Horizontal Tee, 6\" x 4\" (150mm x 100mm), FiberRunner, YL","",4,"Piece","","Panduit.com product page"]
["Fiber Routing",34,"FREC6X4LYL","Fitting, End Cap, 6\" x 4\" (150mm x 100mm), FiberRunner, YL","",4,"Piece","","Panduit.com product page"]
[]
["Fiber Breakout and Splitting"]
["",35,"FLEX1U12","HD Flex 1 RU 12-Port Enclosure","",1,"Piece","","Panduit.com product page"]
["",36,"FHS9N-12-3AP","12F OS2 HD Flex SC/APC Splice Cassette loaded with discrete pigtails","",1,"Piece","","Panduit.com product page"]
["Holds 1:2 Splitters",37,"FLEX4U04","HD Flex 4 RU 4-port enclosure","",8,"Piece","","Panduit.com product page"]
["64 per 4 RU (512 total)",38,"FHP9N-LA1X02","HD Flex PON Splitter Cassette, 1x2, ¾ width, LC/APC to LC/APC","",512,"Piece","","Panduit.com product page"]
["1024 F to Breakouts",39,"F91ERANB1SNM005","OS2 1f 1.6mm PC OFNR SCAPC/LCAPC Std Polarity Std IL 5m","",1024,"Piece","","Panduit.com product page"]
["Breakout 1024",40,"FLEX4U12","HD Flex 4 RU 12-port enclosure","",8,"Piece","","Panduit.com product page"]
["24 per 4 RU",41,"FHS9N-12-3AP","12F OS2 HD Flex SC/APC Splice Cassette loaded with discrete pigtails","",85,"Piece","","Panduit.com product page"]
["",42,"FLEX-PLATE1U","HD Flex Enclosure Trunk Slack Plate - 1RU","",1,"Piece","","Panduit.com product page"]
["",43,"FLEX-PLATE4U","HD Flex Enclosure Trunk Slack Plate - 4RU","",16,"Piece","","Panduit.com product page"]
[]
["Equipment Grounding and Lightning Protection"]
["G&B",44,"GB4B0612TPI-1","Grounding Busbar, BICSI 1/4\" x 4\" x 12\" (6.4mm x 102mm x 305mm)","",1,"Piece","","Panduit.com product page"]
["G&B",45,"RGRB19Y","Grounding Busbar Kits, 19\" (483mm) Lgth, 14 mounting holes, 1/2\" (12.7mm) Hole Spacing","",9,"Kit","","Panduit.com product page"]
["G&B",46,"RGRB19CN","Grounding Busbar Kits, 19\" (483mm) Lgth, 20 mounting holes, 5/8\" (15.9mm) Hole Spacing","",3,"Kit","","Panduit.com product page"]
["G&B",47,"RGEJ1024PFY","Jumper Kits, Equipment Grounding, #10 AWG (6mm²) Jumper; Factory Terminated Both Ends","",52,"Kit","","Panduit.com product page"]
["G&B",48,"CNBK","Bonding Cage Nut Kit","",2,"Kit","","Panduit.com product page"]
["G&B",49,"RGTBSG-C","Bonding Screw, Green","",5,"Piece","","Panduit.com product page"]
["G&B",50,"ACG24K","Armored Cable Grounding Kits","",8,"Kit","","Panduit.com product page"]
["G&B",51,"GJ6288UH","Telecom Equipment Bonding Conductor (TEBC) Kits, Jumper Pre-Terminated on Both Ends","",2,"Kit","","Panduit.com product page"]
["G&B",52,"RGCBNJ460P","Jumper Kits, Common Bonding Network (CBN), #4 AWG (21.2mm²) Jumper, 60 (1.52m) Length","",10,"Kit",1,"Panduit.com product page"]
[]
["Fiber Connectivity and Cable"]
["",53,"FSDR91AY","9um OS2 144 Fiber Indoor Distribution Cable, Riser (OFNR), 900um Buffered Fibers","",1,"Foot","","Panduit.com product page"]
["12 F to DWDM",54,"F913RANANSNM005","OS2 1f 3mm PC OFNR SCAPC/SCAPC Std Polarity Std IL 5m","",12,"Piece",1,"Panduit.com product page"]
["12 F to 3 Routers",55,"F913RANANSNM005","OS2 1f 3mm PC OFNR SCAPC/SCAPC Std Polarity Std IL 5m","",12,"Piece",1,"Panduit.com product page"]
["12 F to BSS/OSS Servers",56,"F913RANANSNM005","OS2 1f 3mm PC OFNR SCAPC/SCAPC Std Polarity Std IL 5m","",12,"Piece",1,"Panduit.com product page"]
["24 F to 1U 16-port OLTs",57,"F913RANANSNM010","OS2 1f 3mm PC OFNR SCAPC/SCAPC Std Polarity Std IL 10m","",24,"Piece",1,"Panduit.com product page"]
["512 F to Splitters",58,"F91ERANB1SNM005","OS2 1f 1.6mm PC OFNR SCAPC/LCAPC Std Polarity Std IL 5m","",512,"Piece","","Panduit.com product page"]
[]
["Cable Management and Identification"]
["Bundling",59,"HLB2S-C0","Hook & Loop Stacked Strip Ties, 7.0L (178mm), .75W (19.1mm), 100 pcs, Black","",10,"Package","","Panduit.com product page"]
["Labeling",60,"MP300","Includes MP300 Printer, 1 Cassette of S100X150VAM, Hard Carrying Case, Li-Ion Battery Pack, Magnetic Attachments, USB Cable, and Power Adapter (MP300-AC). For use in North America","",1,"Piece","","Panduit.com product page"]
["Labeling",61,"T024X000FJM-BK","MP Cassette, Continuous Tape, Polyolefin, .24\" W x 23' L, Black on White","",8,"Piece","","Panduit.com product page"]
["Labeling",62,"T100X000VPM-BK","MP Cassette, Continuous Tape, Vinyl, 1.00\" W x 23' L, Black on White","",4,"Piece","","Panduit.com product page"]
["Labeling",63,"T050X000VPM-BK","MP Cassette, Continuous Tape, Vinyl, .50\" W x 23' L, Black on White","",2,"Piece","","Panduit.com product page"]
["Labeling",64,"S100X125VAM","MP Cassette, Self-Laminating Label, Vinyl, 1.00\" W x 1.25\" H, .38\" Print On Area, Clear/ White","",1,"Piece","","Panduit.com product page"]
["Labeling",65,"S100X075VAM","MP Cassette, Self-Laminating Label, Vinyl, 1.00\" W x .75\" H, .25\" Print On Area, Clear/ White","",8,"Piece","","Panduit.com product page"]
["Notes: 1. Product is non-cancelable and non-returnable"]
[]
["This Bill of Material is provided “AS IS.”  All part numbers, descriptions, and quantities should be verified for suitability prior to purchase and use.  Purchaser assumes all risk and liability of any kind in connection with the use of this Bill of Material.  Applicable part numbers are shown to the nearest purchasable quantity."]

{"sheet":"OSP New Products","index":1,"n_rows":29,"n_cols":4,"rows_kept":29}
[]
[]
[]
[]
[null,"Family","Part Number","Description"]
[null,"Pedestal","HUB-10","10\" PEDESTAL"]
[null,"Pedestal","HUB-10-MB","10\" PEDESTAL WITH UNIVERSAL MOUNTING BRACKET"]
[null,"Pedestal","HUB-8","8\" Pedestal"]
[null,"Pedestal","HUB-8-MB","8\" Pedestal with universal mounting bracket"]
[null,"Pedestal","HUB-S32","32\" PEDESTAL STAKE"]
[null,"Pedestal","HUB-S42","42\" PEDESTAL STAKE"]
[]
[null,"Service Terminal","P-MST-12D-200","Panduit Service Terminal, 12 port,  Dielectric, 200ft"]
[null,"Service Terminal","P-MST-12D-500","Panduit Service Terminal, 12 port,  Dielectric, 500ft"]
[null,"Service Terminal","P-MST-12T-200","Panduit Service Terminal, 12 port,  Tonable, 200ft"]
[null,"Service Terminal","P-MST-12T-500","Panduit Service Terminal, 12 port,  Tonable, 500ft"]
[null,"Service Terminal","P-MST-4D-200","Panduit Service Terminal, 4 port,  Dielectric, 200ft"]
[null,"Service Terminal","P-MST-4D-500","Panduit Service Terminal, 4 port,  Dielectric, 500ft"]
[null,"Service Terminal","P-MST-4T-200","Panduit Service Terminal, 4 port,  Tonable, 200ft"]
[null,"Service Terminal","P-MST-4T-500","Panduit Service Terminal, 4 port,  Tonable, 500ft"]
[null,"Service Terminal","P-MST-8D-200","Panduit Service Terminal, 8 port,  Dielectric, 200ft"]
[null,"Service Terminal","P-MST-8D-500","Panduit Service Terminal, 8 port,  Dielectric, 500ft"]
[null,"Service Terminal","P-MST-8T-200","Panduit Service Terminal, 8 port, Tonable, 200ft"]
[null,"Service Terminal","P-MST-8T-500","Panduit Service Terminal, 8 port, Tonable, 500ft"]
[null,"Service Terminal","P-MST-ASB","Panduit Service Terminal Strand Mounting bracket kit"]
[]
[null,"Splice Closure","OFC24SST","Single Fiber Splice Tray, 24 Ct."]
[null,"Splice Closure","OFC40SST","Single Fiber Splice Tray, 40 Ct."]
[null,"Splice Closure","OFCD6517BF","Dome closure, 6.5\"x17\", w/ single fusion fiber organizer"]